Kastle 2 Alchemist
Release Notes 

kastle2-alchemist-1.7

Changes:
- added Humanize/Swing (MODE + LFO); co-developed with Tomasz Szymanek, Bastl Discord community member
- added assignable LFO MOD destination (in Advanced Settings)
- added MIDI velocity and sustain support
- small fixes


To check the firmware version:
- Boot into Test Mode: Hold the MODE button and turn the power ON.
- Listen to the Headphone Output / Audio Out directly: The unit will announce the firmware version via its voice output.
- Turn power OFF and ON to exit the test mode

HOW TO UPDATE KASTLE 2
1) Connect the Kastle 2 with a USB-C cable to your computer
2) Turn OFF the power switch (left)
3) Hold SHIFT and turn ON the power switch (right)
4) Kastle 2 will boot into Update Mode (no sound)
5) Copy the firmware .uf2 file to the RPI-RP2 disk showing on your computer.

HOW TO UPDATE CITADEL
1) Disconnect the Citadel module from your Eurorack power!
2) Connect the Citadel with a USB-C cable to your computer while holding the SHIFT button.
3) The Citadel will boot into Update Mode (no sound)
4) Copy the firmware .uf2 file to the RPI-RP2 disk showing on your computer.

Note: Depending on the .uf2 firmware file size, the upload can usually take up to 2 minutes or more.